## Chapter 37 Photographic or Cinematographic Goods

### Chapter Notes

1. This chapter does not cover waste or scrap.

2. In this chapter, the word 'photographic' relates to the process by which visible images are formed, directly or indirectly, by the action of light or other forms of radiation on photosensitive surfaces.

### Additional notes

1. In the case of sound films imported in two bands (the band bearing only the images and the band used for recording the sound), each band is to be classified in its appropriate heading.

2. The expression 'newsreels' (subheading 3706 90 52) is to be taken to apply to films of length of less than 330m, and depicting current events of a political, sporting, military, scientific, literary, folkloric, touristic, society, etc., nature.

| Classification | Description |
| --- | --- |
| **3701** | **Photographic plates and film in the flat, sensitised, unexposed, of any material other than paper, paperboard or textiles; instant print film in the flat, sensitised, unexposed, whether or not in packs** |
| **3701 10** | **- For X-ray** |
| **3701 20** | **- Instant print film** |
| **3701 30** | **- Other plates and film, with any side exceeding 255 mm** |
| **3701 30 00 20** | - - Photosensitive plate consisting of a photopolymer layer on a polyester foil of a total thickness of more than 0,43 mm but not more than 3,18 mm |
| **3701 30 00 30** | - - Relief printing plate, of a kind used for printing on newsprint, consisting of a metal substrate coated with a photopolymer layer of a thickness of 0,15 mm or more but not more than 0,8 mm, not covered with a release film, of a total thickness of not more than 1 mm |
| **3701 30 00 90** | - - Other |
|  | **- Other** |
| **3701 91** | - - For colour photography (polychrome) |
| **3701 99** | - - Other |
| **3701 99 00 10** | - - - Plate of quartz or of glass, covered with a film of chromium and coated with a photosensitive or electron-sensitive resin, of a kind used for goods of heading 8541 or 8542 |
| **3701 99 00 90** | - - - Other |
| **3702** | **Photographic film in rolls, sensitised, unexposed, of any material other than paper, paperboard or textiles; instant print film in rolls, sensitised, unexposed** |
| **3702 10** | **- For X-ray** |
|  | **- Other film, without perforations, of a width not exceeding 105 mm** |
| **3702 31** | - - For colour photography (polychrome) |
| **3702 31 91** | - - - Colour negative film:- of a width of 75 mm or more but not exceeding 105 mm and- of a length of 100 m or morefor the manufacture of instant-picture film-packs |
| **3702 31 97** | - - - Other |
| **3702 32** | - - Other, with silver halide emulsion |
|  | - - - Of a width not exceeding 35 mm |
| **3702 32 10** | - - - - Microfilm; film for the graphic arts |
| **3702 32 20** | - - - - Other |
| **3702 32 85** | - - - Of a width exceeding 35 mm |
| **3702 39** | - - Other |
|  | **- Other film, without perforations, of a width exceeding 105 mm** |
| **3702 41** | - - Of a width exceeding 610 mm and of a length exceeding 200 m, for colour photography (polychrome) |
| **3702 42** | - - Of a width exceeding 610 mm and of a length exceeding 200 m, other than for colour photography |
| **3702 43** | - - Of a width exceeding 610 mm and of a length not exceeding 200 m |
| **3702 44** | - - Of a width exceeding 105 mm but not exceeding 610 mm |
|  | **- Other film, for colour photography (polychrome)** |
| **3702 52** | - - Of a width not exceeding 16 mm |
| **3702 53** | - - Of a width exceeding 16 mm but not exceeding 35 mm and of a length not exceeding 30 m, for slides |
| **3702 54** | - - Of a width exceeding 16 mm but not exceeding 35 mm and of a length not exceeding 30 m, other than for slides |
| **3702 55** | - - Of a width exceeding 16 mm but not exceeding 35 mm and of a length exceeding 30 m |
| **3702 56** | - - Of a width exceeding 35 mm |
|  | **- Other** |
| **3702 96** | - - Of a width not exceeding 35 mm and of a length not exceeding 30 m |
| **3702 96 10** | - - - Microfilm; film for the graphic arts |
| **3702 96 90** | - - - Other |
| **3702 97** | - - Of a width not exceeding 35 mm and of a length exceeding 30 m |
| **3702 97 10** | - - - Microfilm; film for the graphic arts |
| **3702 97 90** | - - - Other |
| **3702 98** | - - Of a width exceeding 35 mm |
| **3703** | **Photographic paper, paperboard and textiles, sensitised, unexposed** |
| **3703 10** | **- In rolls of a width exceeding 610 mm** |
| **3703 20** | **- Other, for colour photography (polychrome)** |
| **3703 90** | **- Other** |
| **3704** | **Photographic plates, film, paper, paperboard and textiles, exposed but not developed** |
| **3704 00 10** | **- Plates and film** |
| **3704 00 90** | **- Other** |
| **3705** | **Photographic plates and film, exposed and developed, other than cinematographic film** |
| **3705 00 10** | **- For offset reproduction** |
| **3705 00 90** | **- Other** |
| **3706** | **Cinematographic film, exposed and developed, whether or not incorporating soundtrack or consisting only of soundtrack** |
| **3706 10** | **- Of a width of 35 mm or more** |
| **3706 10 20** | - - Consisting only of soundtrack; negatives; intermediate positives |
| **3706 10 99** | - - Other positives |
| **3706 90** | **- Other** |
| **3706 90 52** | - - Consisting only of soundtrack; negatives; intermediate positives; newsreels |
|  | - - Other, of a width of |
| **3706 90 91** | - - - Less than 10 mm |
| **3706 90 99** | - - - 10 mm or more |
| **3707** | **Chemical preparations for photographic uses (other than varnishes, glues, adhesives and similar preparations); unmixed products for photographic uses, put up in measured portions or put up for retail sale in a form ready for use** |
| **3707 10** | **- Sensitising emulsions** |
| **3707 10 00 10** | - - Photosensitive emulsion for the sensitization of silicon discs |
| **3707 10 00 15** | - - Sensitising emulsion consisting of:   - by weight not more than 12 % of diazooxonapthtalenesulphonic acid ester   - phenolic resins in a solution containing at least 2-methoxy-1-methylethyl acetate or ethyl lactate or methyl 3-methoxypropionate or 2-heptanone |
| **3707 10 00 25** | - - Sensitising emulsion containing:   - phenolic or acrylic resins   - a maximum 2 % by weight of light sensitive acid precursor, in a solution containing 2-methoxy-1-methylethyl acetate or ethyl lactate |
| **3707 10 00 30** | - - Preparation based on photosensitive acrylic containing polymer, containing colour pigments, 2-methoxy-1-methylethylacetate and cyclohexanone and whether or not containing ethyl-3-ethoxypropionate |
| **3707 10 00 35** | - - Sensitising emulsion or preparation containing one or more of:  • acrylate polymers • methacrylate polymers  • derivatives of styrene polymers  containing by weight not more than 7% of photosensitive acid precursors, dissolved in an organic solvent containing at least 2-methoxy-1-methylethyl acetate |
| **3707 10 00 40** | - - Sensitising emulsion, containing:   - not more than 10 % by weight of naphthoquinonediazide esters,   - 2 % or more but not more than 35 % by weight of copolymers of hydroxystyrene   - not more than 7 % by weight of epoxy-containing derivatives dissolved in 1-ethoxy-2-propyl acetate and/or ethyl lactate |
| **3707 10 00 45** | - - Photosensitive emulsion consisting of cyclized polyisoprene containing:   - 55 % or more but not more than 75 % by weight of xylene and   - 12 % or more but not more than 18 % by weight of ethylbenzene |
| **3707 10 00 50** | - - Photosensitive emulsion containing by weight:   - 20 % or more but not more than 45 % of copolymers of acrylates and/or methacrylates and hydroxystyrene derivatives,   - 25 % or more but not more than 50 % of organic solvent containing at least ethyl lactate and/or propylene glycolmethylether acetate,   - 5 % or more but not more than 30 % of acrylates,   - not more than 12 % of a photoinitiator |
| **3707 10 00 55** | - - Dielectric coating, buffering mechanical stress, consisting of a radically photopatternable polyamide-precursor with unsaturated carbon in the side-chains which is convertible into a polyimide, in form of a solution from N-methyl-2-pyrrolidone or N-ethyl-2-pyrrolidon with a polymer content by weight 10 % or more |
| **3707 10 00 60** | - - Sensitising emulsion, containing by weight: - not more than 5 % of photoacid generator, - 2 % or more but not more than 50 % of phenolic resins, and - not more than 7 % of epoxy-containing derivatives, dissolved in heptan-2-one and/or ethyllactate |
| **3707 10 00 90** | - - Other |
| **3707 90** | **- Other** |
|  | - - Developers and fixers |
| **3707 90 21** | - - - Thermoplastic or electrostatic toner cartridges (without moving parts) for insertion into apparatus of subheadings 8443 31, 8443 32 or 8443 39 |
| **3707 90 29** | - - - Other |
| **3707 90 29 10** | - - - - Dry ink powder or toner blend, consisting of a copolymer of styrene and butyl acrylate and either magnetite or carbon black, for use as a developer in the manufacture of cartridges for facsimile machines, computer printers or copiers |
| **3707 90 29 20** | - - - - Dry ink powder or toner blend, based on a polyol resin, for use as a developer in the manufacture of cartridges for facsimile machines, computer printers or copiers |
| **3707 90 29 40** | - - - - Dry ink powder or toner blend, based on a polyester resin, manufactured by a polymerisation process, for use as a developer in the manufacture of cartridges for facsimile machines, computer printers or copiers |
| **3707 90 29 50** | - - - - Dry ink powder or toner blend, consisting of:    - styrene acrylate/butadiene copolymer   - either carbon black or an organic pigment   - whether or not containing polyolefin or amorphous silica  for use as a developer in the manufacturing of ink/toner filled bottles or cartridges for facsimile machines, computer printers and copiers |
| **3707 90 29 90** | - - - - Other |
| **3707 90 90** | - - Other |