# Section XV Base metals and articles of base metal

## Chapter 72 Iron and Steel

| Commodity code | Duty expression | Notes | Description |
| --- | --- | --- | --- |
| **7200** |  |  | **IRON AND STEEL** |
|  |  |  | **I. PRIMARY MATERIALS; PRODUCTS IN GRANULAR OR POWDER FORM** |
| **7201** |  |  | **Pig iron and spiegeleisen in pigs, blocks or other primary forms** |
| **7201 10** |  |  | **- Non-alloy pig iron containing by weight 0,5% or less of phosphorus** |
|  |  |  | - - Containing by weight not less than 0,4% of manganese |
| **7201 10 11** |  |  | - - - Containing by weight 1% or less of silicon |
| **7201 10 11 10** | 1.7% |  | - - - - Pig iron ingots with a length of not more than 350 mm, a width of not more than 150 mm, a height of not more than 150 mm |
| **7201 10 11 90** |  |  | - - - - Other |
| **7201 10 19 00** | 1.7% |  | - - - Containing by weight more than 1% of silicon |
| **7201 10 30** |  |  | - - Containing by weight not less than 0,1% but less than 0,4% of manganese |
| **7201 10 30 10** | 1.7% |  | - - - Pig iron ingots with a length of not more than 350 mm, a width of not more than 150 mm, a height of not more than 150 mm, containing by weight not more than 1% of silicon |
| **7201 10 30 90** |  |  | - - - Other |
| **7201 10 90 00** | 0.0% |  | - - Containing by weight less than 0,1% of manganese |
| **7201 20 00 00** | 2.2% |  | **- Non-alloy pig iron containing by weight more than 0,5% of phosphorus** |
| **7201 50** |  |  | **- Alloy pig iron; spiegeleisen** |
| **7201 50 10 00** | 0.0% |  | - - Alloy pig iron containing by weight not less than 0,3% but not more than 1% of titanium and not less than 0,5% but not more than 1% of vanadium |
| **7201 50 90 00** | 1.7% |  | - - Other |
| **7202** |  |  | **Ferro-alloys** |
|  |  |  | **- Ferro-manganese** |
| **7202 11** |  |  | - - Containing by weight more than 2% of carbon |
| **7202 11 20 00** | 2.7% |  | - - - With a granulometry not exceeding 5 mm and a manganese content by weight exceeding 65% |
| **7202 11 80 00** |  |  | - - - Other |
| **7202 19 00 00** | 2.7% |  | - - Other |
|  |  |  | **- Ferro-silicon** |
| **7202 21 00 00** | 5.7% |  | - - Containing by weight more than 55% of silicon |
| **7202 29** |  |  | - - Other |
| **7202 29 10 00** | 5.7% |  | - - - Containing by weight 4% or more but not more than 10% of magnesium |
| **7202 29 90 00** |  |  | - - - Other |
| **7202 30 00 00** | 3.7% |  | **- Ferro-silico-manganese** |
|  |  |  | **- Ferro-chromium** |
| **7202 41** |  |  | - - Containing by weight more than 4% of carbon |
| **7202 41 10 00** | 4.0% |  | - - - Containing by weight more than 4% but not more than 6% of carbon |
| **7202 41 90 00** |  |  | - - - Containing by weight more than 6% of carbon |
| **7202 49** |  |  | - - Other |
| **7202 49 10** |  |  | - - - Containing by weight not more than 0,05% of carbon |
| **7202 49 10 20** | 7.0% |  | - - - - Containing by weight more than 30% but not more than 90% of chromium (super-refined ferrochromium) |
| **7202 49 10 90** |  |  | - - - - Other |
| **7202 49 50** |  |  | - - - Containing by weight more than 0,05% but not more than 0,5% of carbon |
|  |  |  | - - - - With a chromium content by weight of 30% and more |
| **7202 49 50 11** | 7.0% |  | - - - - - Containing by weight not more than 0,1% of carbon and more than 30% but not more than 90% of chromium (super-refined ferrochromium) |
| **7202 49 50 19** |  |  | - - - - - Other |
| **7202 49 50 90** |  |  | - - - - Other |
| **7202 49 90** |  |  | - - - Containing by weight more than 0,5% but not more than 4% of carbon |
| **7202 49 90 10** |  |  | - - - - Containing 1,5% or more but not more than 4% by weight of carbon and not more than 70% of chromium |
| **7202 49 90 90** |  |  | - - - - Other |
| **7202 50 00 00** | 2.7% |  | **- Ferro-silico-chromium** |
| **7202 60 00 00** | 0.0% |  | **- Ferro-nickel** |
| **7202 70 00 00** | 2.7% |  | **- Ferro-molybdenum** |
| **7202 80 00 00** | 0.0% |  | **- Ferro-tungsten and ferro-silico-tungsten** |
|  |  |  | **- Other** |
| **7202 91 00 00** | 2.7% |  | - - Ferro-titanium and ferro-silico-titanium |
| **7202 92 00 00** | 2.7% |  | - - Ferro-vanadium |
| **7202 93 00 00** | 0.0% |  | - - Ferro-niobium |
| **7202 99** |  |  | - - Other |
| **7202 99 10 00** | 0.0% |  | - - - Ferro-phosphorus |
| **7202 99 30 00** | 2.7% |  | - - - Ferro-silico-magnesium |
| **7202 99 80** |  |  | - - - Other |
| **7202 99 80 10** | 2.7% |  | - - - - Ferro-dysprosium, containing by weight: - 78% or more of dysprosium and - 18% or more but no more than 22% of iron |
| **7202 99 80 90** |  |  | - - - - Other |
| **7203** |  |  | **Ferrous products obtained by direct reduction of iron ore and other spongy ferrous products, in lumps, pellets or similar forms; iron having a minimum purity by weight of 99,94%, in lumps, pellets or similar forms** |
| **7203 10 00 00** | 0.0% |  | **- Ferrous products obtained by direct reduction of iron ore** |
| **7203 90 00 00** |  |  | **- Other** |
| **7204** |  |  | **Ferrous waste and scrap; remelting scrap ingots of iron or steel** |
| **7204 10 00 00** | 0.0% |  | **- Waste and scrap of cast iron** |
|  |  |  | **- Waste and scrap of alloy steel** |
| **7204 21** |  |  | - - Of stainless steel |
| **7204 21 10** |  |  | - - - Containing by weight 8% or more of nickel |
| **7204 21 10 10** | 0.0% |  | - - - - Scrap |
| **7204 21 10 90** |  |  | - - - - Other |
| **7204 21 90** |  |  | - - - Other |
| **7204 21 90 10** |  |  | - - - - Scrap |
| **7204 21 90 90** |  |  | - - - - Other |
| **7204 29** |  |  | - - Other |
| **7204 29 00 10** |  |  | - - - Scrap |
| **7204 29 00 90** |  |  | - - - Other |
| **7204 30** |  |  | **- Waste and scrap of tinned iron or steel** |
| **7204 30 00 10** |  |  | - - Scrap |
| **7204 30 00 90** |  |  | - - Other |
|  |  |  | **- Other waste and scrap** |
| **7204 41** |  |  | - - Turnings, shavings, chips, milling waste, sawdust, filings, trimmings and stampings, whether or not in bundles |
| **7204 41 10** |  |  | - - - Turnings, shavings, chips, milling waste, sawdust and filings |
| **7204 41 10 10** |  |  | - - - - Scrap |
| **7204 41 10 90** |  |  | - - - - Other |
|  |  |  | - - - Trimmings and stampings |
| **7204 41 91** |  |  | - - - - In bundles |
| **7204 41 91 10** | 0.0% |  | - - - - - Scrap |
| **7204 41 91 90** |  |  | - - - - - Other |
| **7204 41 99** |  |  | - - - - Other |
| **7204 41 99 10** |  |  | - - - - - Scrap |
| **7204 41 99 90** |  |  | - - - - - Other |
| **7204 49** |  |  | - - Other |
| **7204 49 10** |  |  | - - - Fragmentised (shredded) |
| **7204 49 10 10** |  |  | - - - - Scrap |
| **7204 49 10 90** |  |  | - - - - Other |
|  |  |  | - - - Other |
| **7204 49 30** |  |  | - - - - In bundles |
| **7204 49 30 10** |  |  | - - - - - Scrap |
| **7204 49 30 90** |  |  | - - - - - Other |
| **7204 49 90** |  |  | - - - - Other |
| **7204 49 90 10** |  |  | - - - - - Scrap |
| **7204 49 90 90** |  |  | - - - - - Other |
| **7204 50 00 00** |  |  | **- Remelting scrap ingots** |
| **7205** |  |  | **Granules and powders, of pig iron, spiegeleisen, iron or steel** |
| **7205 10 00 00** | 0.0% |  | **- Granules** |
|  |  |  | **- Powders** |
| **7205 21 00 00** | 0.0% |  | - - Of alloy steel |
| **7205 29 00 00** |  |  | - - Other |
|  |  |  | **II. IRON AND NON-ALLOY STEEL** |
| **7206** |  |  | **Iron and non-alloy steel in ingots or other primary forms (excluding iron of heading 7203)** |
| **7206 10 00 00** | 0.0% |  | **- Ingots** |
| **7206 90 00 00** |  |  | **- Other** |
| **7207** |  |  | **Semi-finished products of iron or non-alloy steel** |
|  |  |  | **- Containing by weight less than 0,25% of carbon** |
| **7207 11** |  |  | - - Of rectangular (including square) cross-section, the width measuring less than twice the thickness |
|  |  |  | - - - Rolled or obtained by continuous casting |
| **7207 11 11 00** | 0.0% |  | - - - - Of free-cutting steel |
|  |  |  | - - - - Other |
| **7207 11 14 00** | 0.0% |  | - - - - - Of a thickness not exceeding 130 mm |
| **7207 11 16 00** |  |  | - - - - - Of a thickness exceeding 130 mm |
| **7207 11 90 00** |  |  | - - - Forged |
| **7207 12** |  |  | - - Other, of rectangular (other than square) cross-section |
| **7207 12 10 00** |  |  | - - - Rolled or obtained by continuous casting |
| **7207 12 90 00** |  |  | - - - Forged |
| **7207 19** |  |  | - - Other |
|  |  |  | - - - Of circular or polygonal cross-section |
| **7207 19 12 00** |  |  | - - - - Rolled or obtained by continuous casting |
| **7207 19 19 00** |  |  | - - - - Forged |
| **7207 19 80** |  |  | - - - Other |
| **7207 19 80 10** |  |  | - - - - Blanks for angles, shapes and sections, rolled or obtained by continuous casting |
| **7207 19 80 90** |  |  | - - - - Other |
| **7207 20** |  |  | **- Containing by weight 0,25% or more of carbon** |
|  |  |  | - - Of rectangular (including square) cross-section, the width measuring less than twice the thickness |
|  |  |  | - - - Rolled or obtained by continuous casting |
| **7207 20 11 00** |  |  | - - - - Of free-cutting steel |
|  |  |  | - - - - Other, containing by weight |
| **7207 20 15 00** |  |  | - - - - - 0,25% or more but less than 0,6% of carbon |
| **7207 20 17 00** |  |  | - - - - - 0,6% or more of carbon |
| **7207 20 19 00** |  |  | - - - Forged |
|  |  |  | - - Other, of rectangular (other than square) cross-section |
| **7207 20 32 00** |  |  | - - - Rolled or obtained by continuous casting |
| **7207 20 39 00** |  |  | - - - Forged |
|  |  |  | - - Of circular or polygonal cross-section |
| **7207 20 52 00** |  |  | - - - Rolled or obtained by continuous casting |
| **7207 20 59 00** |  |  | - - - Forged |
| **7207 20 80** |  |  | - - Other |
| **7207 20 80 10** |  |  | - - - Blanks for angles, shapes and sections, rolled or obtained by continuous casting |
| **7207 20 80 90** |  |  | - - - Other |
| **7208** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of 600 mm or more, hot-rolled, not clad, plated or coated** |
| **7208 10 00 00** | 0.0% |  | **- In coils, not further worked than hot-rolled, with patterns in relief** |
|  |  |  | **- Other, in coils, not further worked than hot-rolled, pickled** |
| **7208 25 00 00** | 0.0% |  | - - Of a thickness of 4.75 mm or more |
| **7208 26 00 00** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7208 27 00 00** |  |  | - - Of a thickness of less than 3 mm |
|  |  |  | **- Other, in coils, not further worked than hot-rolled** |
| **7208 36 00 00** |  |  | - - Of a thickness exceeding 10 mm |
| **7208 37** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7208 37 00 10** | 0.0% |  | - - - Intended for re-rolling |
| **7208 37 00 90** |  |  | - - - Other |
| **7208 38** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7208 38 00 10** |  |  | - - - Intended for re-rolling |
| **7208 38 00 90** |  |  | - - - Other |
| **7208 39** |  |  | - - Of a thickness of less than 3 mm |
| **7208 39 00 10** |  |  | - - - Intended for re-rolling |
| **7208 39 00 90** |  |  | - - - Other |
| **7208 40** |  |  | **- Not in coils, not further worked than hot-rolled, with patterns in relief** |
| **7208 40 00 10** |  |  | - - Of a thickness of 2 mm or more |
| **7208 40 00 90** |  |  | - - Of a thickness of less than 2 mm |
|  |  |  | **- Other, not in coils, not further worked than hot-rolled** |
| **7208 51** |  |  | - - Of a thickness exceeding 10 mm |
| **7208 51 20** |  |  | - - - Of a thickness exceeding 15 mm |
| **7208 51 20 10** | 0.0% |  | - - - - Of non-alloy steel, excluding tool steel |
| **7208 51 20 90** |  |  | - - - - Other |
|  |  |  | - - - Of a thickness exceeding 10 mm but not exceeding 15 mm, of a width of |
| **7208 51 91** |  |  | - - - - 2 050 mm or more |
| **7208 51 91 10** | 0.0% |  | - - - - - Of non-alloy steel, excluding tool steel |
| **7208 51 91 90** |  |  | - - - - - Other |
| **7208 51 98** |  |  | - - - - Less than 2 050 mm |
| **7208 51 98 10** |  |  | - - - - - Of non-alloy steel, excluding tool steel |
| **7208 51 98 90** |  |  | - - - - - Other |
| **7208 52** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7208 52 10 00** |  |  | - - - Rolled on four faces or in a closed box pass, of a width not exceeding 1 250 mm |
|  |  |  | - - - Other, of a width of |
| **7208 52 91** |  |  | - - - - 2 050 mm or more |
| **7208 52 91 10** |  |  | - - - - - Of non-alloy steel, excluding tool steel |
| **7208 52 91 90** |  |  | - - - - - Other |
| **7208 52 99 00** |  |  | - - - - Less than 2 050 mm |
| **7208 53** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7208 53 10 00** |  |  | - - - Rolled on four faces or in a closed box pass, of a width not exceeding 1 250 mm and of a thickness of 4 mm or more |
| **7208 53 90 00** |  |  | - - - Other |
| **7208 54 00 00** |  |  | - - Of a thickness of less than 3 mm |
| **7208 90** |  |  | **- Other** |
| **7208 90 20** |  |  | - - Perforated |
| **7208 90 20 10** |  |  | - - - Of non-alloy steel, excluding tool steel, of a thickness exceeding 10 mm or of a thickness of 4.75 mm or more but not exceeding 10 mm and of a width of 2 050 mm or more |
| **7208 90 20 90** |  |  | - - - Other |
| **7208 90 80** |  |  | - - Other |
| **7208 90 80 10** |  |  | - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7208 90 80 20** |  |  | - - - Of non-alloy steel, excluding tool steel, of a thickness exceeding 10 mm or of a thickness of 4.75 mm or more but not exceeding 10 mm and of a width of 2 050 mm or more |
| **7208 90 80 90** |  |  | - - - Other |
| **7209** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of 600 mm or more, cold-rolled (cold-reduced), not clad, plated or coated** |
|  |  |  | **- In coils, not further worked than cold-rolled (cold-reduced)** |
| **7209 15** |  |  | - - Of a thickness of 3 mm or more |
| **7209 15 00 10** | 0.0% |  | - - - 'Electrical' |
| **7209 15 00 90** |  |  | - - - Other |
| **7209 16** |  |  | - - Of a thickness exceeding 1 mm but less than 3 mm |
| **7209 16 10 00** |  |  | - - - 'Electrical' |
| **7209 16 90 00** |  |  | - - - Other |
| **7209 17** |  |  | - - Of a thickness of 0.5 mm or more but not exceeding 1 mm |
| **7209 17 10 00** |  |  | - - - 'Electrical' |
| **7209 17 90 00** |  |  | - - - Other |
| **7209 18** |  |  | - - Of a thickness of less than 0.5 mm |
| **7209 18 10 00** |  |  | - - - 'Electrical' |
|  |  |  | - - - Other |
| **7209 18 91 00** | 0.0% |  | - - - - Of a thickness of 0.35 mm or more but less than 0.5 mm |
| **7209 18 99** |  |  | - - - - Of a thickness of less than 0.35 mm |
| **7209 18 99 10** | 0.0% |  | - - - - - Annealed (known as 'black plates') |
| **7209 18 99 90** |  |  | - - - - - Other |
|  |  |  | **- Not in coils, not further worked than cold-rolled (cold-reduced)** |
| **7209 25** |  |  | - - Of a thickness of 3 mm or more |
| **7209 25 00 10** |  |  | - - - 'Electrical' |
| **7209 25 00 90** |  |  | - - - Other |
| **7209 26** |  |  | - - Of a thickness exceeding 1 mm but less than 3 mm |
| **7209 26 10 00** |  |  | - - - 'Electrical' |
| **7209 26 90 00** |  |  | - - - Other |
| **7209 27** |  |  | - - Of a thickness of 0.5 mm or more but not exceeding 1 mm |
| **7209 27 10 00** |  |  | - - - 'Electrical' |
| **7209 27 90 00** |  |  | - - - Other |
| **7209 28** |  |  | - - Of a thickness of less than 0.5 mm |
| **7209 28 10 00** |  |  | - - - 'Electrical' |
| **7209 28 90 00** |  |  | - - - Other |
| **7209 90** |  |  | **- Other** |
| **7209 90 20 00** |  |  | - - Perforated |
| **7209 90 80** |  |  | - - Other |
| **7209 90 80 10** |  |  | - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7209 90 80 90** |  |  | - - - Other |
| **7210** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of 600 mm or more, clad, plated or coated** |
|  |  |  | **- Plated or coated with tin** |
| **7210 11** |  |  | - - Of a thickness of 0.5 mm or more |
| **7210 11 00 10** | 0.0% |  | - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 11 00 90** |  |  | - - - Other |
| **7210 12** |  |  | - - Of a thickness of less than 0.5 mm |
| **7210 12 20** |  |  | - - - Tinplate |
| **7210 12 20 10** | 0.0% |  | - - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 12 20 90** |  |  | - - - - Other |
| **7210 12 80** |  |  | - - - Other |
| **7210 12 80 10** |  |  | - - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 12 80 90** |  |  | - - - - Other |
| **7210 20** |  |  | **- Plated or coated with lead, including terne-plate** |
| **7210 20 00 10** |  |  | - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 20 00 90** |  |  | - - Other |
| **7210 30** |  |  | **- Electrolytically plated or coated with zinc** |
| **7210 30 00 10** |  |  | - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 30 00 90** |  |  | - - Other |
|  |  |  | **- Otherwise plated or coated with zinc** |
| **7210 41** |  |  | - - Corrugated |
| **7210 41 00 20** |  |  | - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7210 41 00 80** |  |  | - - - Other |
| **7210 49** |  |  | - - Other |
| **7210 49 00 20** |  |  | - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7210 49 00 80** |  |  | - - - Other |
| **7210 50** |  |  | **- Plated or coated with chromium oxides or with chromium and chromium oxides** |
| **7210 50 00 10** |  |  | - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 50 00 90** |  |  | - - Other |
|  |  |  | **- Plated or coated with aluminium** |
| **7210 61** |  |  | - - Plated or coated with aluminium-zinc alloys |
| **7210 61 00 20** |  |  | - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7210 61 00 80** |  |  | - - - Other |
| **7210 69** |  |  | - - Other |
| **7210 69 00 20** |  |  | - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7210 69 00 80** |  |  | - - - Other |
| **7210 70** |  |  | **- Painted, varnished or coated with plastics** |
| **7210 70 10** |  |  | - - Tinplate, varnished; products, plated or coated with chromium oxides or with chromium and chromium oxides, varnished |
| **7210 70 10 10** |  |  | - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 70 10 90** |  |  | - - - Other |
| **7210 70 80** |  |  | - - Other |
|  |  |  | - - - Not further worked than surface-treated or simply cut into shapes other than rectangular (including square) |
| **7210 70 80 11** |  |  | - - - - Of non-alloy steel, painted, varnished or coated with plastics on at least one side, excluding products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70 % or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7210 70 80 19** |  |  | - - - - Other |
|  |  |  | - - - Other |
| **7210 70 80 91** |  |  | - - - - Of non-alloy steel, painted, varnished or coated with plastics on at least one side, excluding products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70 % or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7210 70 80 99** |  |  | - - - - Other |
| **7210 90** |  |  | **- Other** |
| **7210 90 30** |  |  | - - Clad |
| **7210 90 30 10** |  |  | - - - Not further worked than surface-treated, including cladding, or simply cut into shapes other than rectangular (including square) |
| **7210 90 30 90** |  |  | - - - Other |
| **7210 90 40** |  |  | - - Tinned and printed |
| **7210 90 40 10** |  |  | - - - Not further worked than surface-treated, including cladding, or simply cut into shapes other than rectangular (including square) |
| **7210 90 40 90** |  |  | - - - Other |
| **7210 90 80** |  |  | - - Other |
| **7210 90 80 10** |  |  | - - - Silvered, gilded, platinium-plated or enamelled |
|  |  |  | - - - Other |
| **7210 90 80 91** |  |  | - - - - Not further worked than surface-treated, including cladding, or simply cut into shapes other than rectangular (including square) |
| **7210 90 80 99** |  |  | - - - - Other |
| **7211** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of less than 600 mm, not clad, plated or coated** |
|  |  |  | **- Not further worked than hot-rolled** |
| **7211 13 00 00** | 0.0% |  | - - Rolled on four faces or in a closed box pass, of a width exceeding 150 mm and a thickness of not less than 4 mm, not in coils and without patterns in relief |
| **7211 14** |  |  | - - Other, of a thickness of 4.75 mm or more |
| **7211 14 00 10** | 0.0% |  | - - - Of a width exceeding 500 mm |
| **7211 14 00 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7211 19** |  |  | - - Other |
| **7211 19 00 10** |  |  | - - - Of a width exceeding 500 mm |
| **7211 19 00 90** |  |  | - - - Of a width not exceeding 500 mm |
|  |  |  | **- Not further worked than cold-rolled (cold-reduced)** |
| **7211 23** |  |  | - - Containing by weight less than 0,25% of carbon |
| **7211 23 20** |  |  | - - - 'Electrical' |
| **7211 23 20 10** | 0.0% |  | - - - - Of a width exceeding 500 mm |
| **7211 23 20 90** |  |  | - - - - Of a width not exceeding 500 mm |
|  |  |  | - - - Other |
| **7211 23 30** |  |  | - - - - Of a thickness of 0.35 mm or more |
| **7211 23 30 10** | 0.0% |  | - - - - - Of a width exceeding 500 mm |
|  |  |  | - - - - - Of a width not exceeding 500 mm |
| **7211 23 30 91** | 0.0% |  | - - - - - - In coils intended for the manufacture of tinplate |
| **7211 23 30 99** |  |  | - - - - - - Other |
| **7211 23 80** |  |  | - - - - Of a thickness of less than 0.35 mm |
|  |  |  | - - - - - Of a width exceeding 500 mm |
| **7211 23 80 11** |  |  | - - - - - - In coils, annealed (known as 'black plates') |
| **7211 23 80 19** |  |  | - - - - - - Other |
|  |  |  | - - - - - Of a width not exceeding 500 mm |
|  |  |  | - - - - - - In coils intended for the manufacture of tinplate |
| **7211 23 80 93** | 0.0% |  | - - - - - - - Annealed (known as 'black plates') |
| **7211 23 80 95** |  |  | - - - - - - - Other |
|  |  |  | - - - - - - Other |
| **7211 23 80 97** |  |  | - - - - - - - In coils, annealed (known as 'black plates') |
| **7211 23 80 99** |  |  | - - - - - - - Other |
| **7211 29** |  |  | - - Other |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7211 29 00 11** |  |  | - - - - 'Electrical' |
| **7211 29 00 19** |  |  | - - - - Other |
|  |  |  | - - - Of a width not exceeding 500 mm |
| **7211 29 00 91** |  |  | - - - - 'Electrical' |
| **7211 29 00 99** |  |  | - - - - Other |
| **7211 90** |  |  | **- Other** |
| **7211 90 20 00** |  |  | - - Perforated |
| **7211 90 80** |  |  | - - Other |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7211 90 80 10** |  |  | - - - - Not further worked than surface-treated |
| **7211 90 80 20** |  |  | - - - - Other |
| **7211 90 80 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7212** |  |  | **Flat-rolled products of iron or non-alloy steel, of a width of less than 600 mm, clad, plated or coated** |
| **7212 10** |  |  | **- Plated or coated with tin** |
| **7212 10 10 00** | 0.0% |  | - - Tinplate, not further worked than surface-treated |
| **7212 10 90** |  |  | - - Other |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7212 10 90 11** | 0.0% |  | - - - - Not further worked than surface-treated |
| **7212 10 90 19** |  |  | - - - - Other |
| **7212 10 90 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7212 20** |  |  | **- Electrolytically plated or coated with zinc** |
|  |  |  | - - Of a width exceeding 500 mm |
| **7212 20 00 11** |  |  | - - - Not further worked than surface-treated |
| **7212 20 00 19** |  |  | - - - Other |
| **7212 20 00 90** |  |  | - - Of a width not exceeding 500 mm |
| **7212 30** |  |  | **- Otherwise plated or coated with zinc** |
| **7212 30 00 20** |  |  | - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7212 30 00 80** |  |  | - - Other |
| **7212 40** |  |  | **- Painted, varnished or coated with plastics** |
| **7212 40 20** |  |  | - - Tinplate, not further worked than varnished; products, plated or coated with chromium oxides or with chromium and chromium oxides, varnished |
| **7212 40 20 10** |  |  | - - - Tinplate, not further worked than varnished |
|  |  |  | - - - Other |
|  |  |  | - - - - Of a width exceeding 500 mm |
| **7212 40 20 91** | 0.0% |  | - - - - - Not further worked than surface-treated |
| **7212 40 20 93** |  |  | - - - - - Other |
| **7212 40 20 99** |  |  | - - - - Of a width not exceeding 500 mm |
| **7212 40 80** |  |  | - - Other |
|  |  |  | - - - Of a width exceeding 500 mm |
|  |  |  | - - - - Not further worked than surface-treated |
| **7212 40 80 01** |  |  | - - - - - Of non-alloy steel, painted, varnished or coated with plastics on at least one side, excluding products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70 % or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7212 40 80 09** |  |  | - - - - - Other |
|  |  |  | - - - - Other |
| **7212 40 80 21** |  |  | - - - - - Of non-alloy steel, painted, varnished or coated with plastics on at least one side, excluding so-called 'sandwich panels' of a kind used for building applications and consisting of two outer metal sheets with a stabilising core of insulation material sandwiched between them, and excluding those products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70% or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7212 40 80 29** |  |  | - - - - - Other |
|  |  |  | - - - Of a width not exceeding 500 mm |
| **7212 40 80 91** |  |  | - - - - Of non-alloy steel, painted, varnished or coated with plastics on at least one side, excluding so-called 'sandwich panels' of a kind used for building applications and consisting of two outer metal sheets with a stabilising core of insulation material sandwiched between them, and excluding those products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70% or more of zinc) |
| **7212 40 80 99** |  |  | - - - - Other |
| **7212 50** |  |  | **- Otherwise plated or coated** |
| **7212 50 20** |  |  | - - Plated or coated with chromium oxides or with chromium and chromium oxides |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7212 50 20 11** |  |  | - - - - Not further worked than surface-treated |
| **7212 50 20 19** |  |  | - - - - Other |
| **7212 50 20 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7212 50 30** |  |  | - - Plated or coated with chromium or nickel |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7212 50 30 11** |  |  | - - - - Not further worked than surface-treated |
| **7212 50 30 19** |  |  | - - - - Other |
| **7212 50 30 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7212 50 40** |  |  | - - Plated or coated with copper |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7212 50 40 11** |  |  | - - - - Not further worked than surface-treated |
| **7212 50 40 19** |  |  | - - - - Other |
| **7212 50 40 90** |  |  | - - - Of a width not exceeding 500 mm |
|  |  |  | - - Plated or coated with aluminium |
| **7212 50 61** |  |  | - - - Plated or coated with aluminium-zinc alloys |
| **7212 50 61 20** |  |  | - - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7212 50 61 80** |  |  | - - - - Other |
| **7212 50 69** |  |  | - - - Other |
| **7212 50 69 20** |  |  | - - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7212 50 69 80** |  |  | - - - - Other |
| **7212 50 90** |  |  | - - Other |
|  |  |  | - - - Of a width exceeding 500 mm |
| **7212 50 90 11** |  |  | - - - - Silvered, gilded, platinum-plated or enamelled |
|  |  |  | - - - - Other |
| **7212 50 90 13** |  |  | - - - - - Not further worked than surface-treated |
| **7212 50 90 19** |  |  | - - - - - Other |
| **7212 50 90 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7212 60** |  |  | **- Clad** |
|  |  |  | - - Of a width exceeding 500 mm |
| **7212 60 00 11** |  |  | - - - Not further worked than surface-treated |
| **7212 60 00 19** |  |  | - - - Other |
|  |  |  | - - Of a width not exceeding 500 mm |
|  |  |  | - - - Not further worked than surface-treated |
| **7212 60 00 91** |  |  | - - - - Hot-rolled, not further worked than clad |
| **7212 60 00 93** |  |  | - - - - Other |
| **7212 60 00 99** |  |  | - - - Other |
| **7213** |  |  | **Bars and rods, hot-rolled, in irregularly wound coils, of iron or non-alloy steel** |
| **7213 10 00 00** | 0.0% |  | **- Containing indentations, ribs, grooves or other deformations produced during the rolling process** |
| **7213 20 00 00** |  |  | **- Other, of free-cutting steel** |
|  |  |  | **- Other** |
| **7213 91** |  |  | - - Of circular cross-section measuring less than 14 mm in diameter |
| **7213 91 10 00** | 0.0% |  | - - - Of a type used for concrete reinforcement |
| **7213 91 20 00** |  |  | - - - Of a type used for tyre cord |
|  |  |  | - - - Other |
| **7213 91 41 00** | 0.0% |  | - - - - Containing by weight 0,06% or less of carbon |
| **7213 91 49 00** |  |  | - - - - Containing by weight more than 0,06% but less than 0,25% of carbon |
| **7213 91 70 00** |  |  | - - - - Containing by weight 0,25% or more but not more than 0,75% of carbon |
| **7213 91 90 00** |  |  | - - - - Containing by weight more than 0,75% of carbon |
| **7213 99** |  |  | - - Other |
| **7213 99 10 00** |  |  | - - - Containing by weight less than 0,25% of carbon |
| **7213 99 90 00** |  |  | - - - Containing by weight 0,25% or more of carbon |
| **7214** |  |  | **Other bars and rods of iron or non-alloy steel, not further worked than forged, hot-rolled, hot-drawn or hot-extruded, but including those twisted after rolling** |
| **7214 10** |  |  | **- Forged** |
| **7214 10 00 10** | 0.0% |  | - - Concrete reinforcement bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process; excluding high fatigue performance concrete reinforcement bars and rods, and excluding other long products, such as round bars |
| **7214 10 00 90** |  |  | - - Other |
| **7214 20** |  |  | **- Containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling** |
| **7214 20 00 10** |  |  | - - High fatigue performance concrete reinforcing bars and rods |
|  |  |  | - - Other |
| **7214 20 00 20** | 0.0% |  | - - - Concrete reinforcement bars and rods excluding long products, such as round bars |
| **7214 20 00 80** |  |  | - - - Other |
| **7214 30** |  |  | **- Other, of free-cutting steel** |
| **7214 30 00 10** |  |  | - - Concrete reinforcement bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process; excluding high fatigue performance concrete reinforcement bars and rods, and excluding other long products, such as round bars |
| **7214 30 00 90** |  |  | - - Other |
|  |  |  | **- Other** |
| **7214 91** |  |  | - - Of rectangular (other than square) cross-section |
| **7214 91 10** |  |  | - - - Containing by weight less than 0,25% of carbon |
| **7214 91 10 10** | 0.0% |  | - - - - Concrete reinforcement bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process; excluding high fatigue performance concrete reinforcement bars and rods, and excluding other long products, such as round bars |
| **7214 91 10 90** |  |  | - - - - Other |
| **7214 91 90** |  |  | - - - Containing by weight 0,25% or more of carbon |
| **7214 91 90 10** |  |  | - - - - Concrete reinforcement bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process; excluding high fatigue performance concrete reinforcement bars and rods, and excluding other long products, such as round bars |
| **7214 91 90 90** |  |  | - - - - Other |
| **7214 99** |  |  | - - Other |
|  |  |  | - - - Containing by weight less than 0,25% of carbon |
| **7214 99 10** |  |  | - - - - Of a type used for concrete reinforcement |
| **7214 99 10 10** | 0.0% |  | - - - - - Bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process; excluding high fatigue performance bars and rods, and excluding other long products, such as round bars |
| **7214 99 10 90** |  |  | - - - - - Other |
|  |  |  | - - - - Other, of circular cross-section measuring in diameter |
| **7214 99 31 00** |  |  | - - - - - 80 mm or more |
| **7214 99 39 00** |  |  | - - - - - Less than 80 mm |
| **7214 99 50 00** |  |  | - - - - Other |
|  |  |  | - - - Containing by weight 0,25% or more of carbon |
|  |  |  | - - - - Of a circular cross-section measuring in diameter |
| **7214 99 71 00** |  |  | - - - - - 80 mm or more |
| **7214 99 79 00** |  |  | - - - - - Less than 80 mm |
| **7214 99 95** |  |  | - - - - Other |
| **7214 99 95 10** |  |  | - - - - - Concrete reinforcement bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process; excluding high fatigue performance concrete reinforcement bars and rods, and excluding other long products, such as round bars |
| **7214 99 95 90** |  |  | - - - - - Other |
| **7215** |  |  | **Other bars and rods of iron or non-alloy steel** |
| **7215 10 00 00** | 0.0% |  | **- Of free-cutting steel, not further worked than cold-formed or cold-finished** |
| **7215 50** |  |  | **- Other, not further worked than cold-formed or cold-finished** |
|  |  |  | - - Containing by weight less than 0,25% of carbon |
| **7215 50 11 00** | 0.0% |  | - - - Of rectangular (other than square) cross-section |
| **7215 50 19 00** |  |  | - - - Other |
| **7215 50 80 00** |  |  | - - Containing by weight 0,25% or more of carbon |
| **7215 90** |  |  | **- Other** |
| **7215 90 00 10** |  |  | - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7215 90 00 90** |  |  | - - Other |
| **7216** |  |  | **Angles, shapes and sections of iron or non-alloy steel** |
| **7216 10 00 00** | 0.0% |  | **- U, I or H sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of less than 80 mm** |
|  |  |  | **- L or T sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of less than 80 mm** |
| **7216 21 00 00** | 0.0% |  | - - L sections |
| **7216 22 00 00** |  |  | - - T sections |
|  |  |  | **- U, I or H sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of 80 mm or more** |
| **7216 31** |  |  | - - U sections |
| **7216 31 10 00** | 0.0% |  | - - - Of a height of 80 mm or more but not exceeding 220 mm |
| **7216 31 90 00** |  |  | - - - Of a height exceeding 220 mm |
| **7216 32** |  |  | - - I sections |
|  |  |  | - - - Of a height of 80 mm or more but not exceeding 220 mm |
| **7216 32 11 00** | 0.0% |  | - - - - With parallel flange faces |
| **7216 32 19 00** |  |  | - - - - Other |
|  |  |  | - - - Of a height exceeding 220 mm |
| **7216 32 91 00** |  |  | - - - - With parallel flange faces |
| **7216 32 99 00** |  |  | - - - - Other |
| **7216 33** |  |  | - - H sections |
| **7216 33 10 00** |  |  | - - - Of a height of 80 mm or more but not exceeding 180 mm |
| **7216 33 90 00** |  |  | - - - Of a height exceeding 180 mm |
| **7216 40** |  |  | **- L or T sections, not further worked than hot-rolled, hot-drawn or extruded, of a height of 80 mm or more** |
| **7216 40 10 00** |  |  | - - L sections |
| **7216 40 90 00** |  |  | - - T sections |
| **7216 50** |  |  | **- Other angles, shapes and sections, not further worked than hot-rolled, hot-drawn or extruded** |
| **7216 50 10 00** |  |  | - - With a cross-section which is capable of being enclosed in a square the side of which is 80 mm |
|  |  |  | - - Other |
| **7216 50 91 00** |  |  | - - - Bulb flats |
| **7216 50 99 00** |  |  | - - - Other |
|  |  |  | **- Angles, shapes and sections, not further worked than cold-formed or cold-finished** |
| **7216 61** |  |  | - - Obtained from flat-rolled products |
| **7216 61 10 00** |  |  | - - - C, L, U, Z, omega or open-ended sections |
| **7216 61 90 00** |  |  | - - - Other |
| **7216 69 00 00** |  |  | - - Other |
|  |  |  | **- Other** |
| **7216 91** |  |  | - - Cold-formed or cold-finished from flat-rolled products |
| **7216 91 10 00** |  |  | - - - Profiled (ribbed) sheets |
| **7216 91 80 00** |  |  | - - - Other |
| **7216 99** |  |  | - - Other |
| **7216 99 00 10** |  |  | - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7216 99 00 90** |  |  | - - - Other |
| **7217** |  |  | **Wire of iron or non-alloy steel** |
| **7217 10** |  |  | **- Not plated or coated, whether or not polished** |
|  |  |  | - - Containing by weight less than 0,25% of carbon |
| **7217 10 10 00** | 0.0% |  | - - - With a maximum cross-sectional dimension of less than 0.8 mm |
|  |  |  | - - - With a maximum cross-sectional dimension of 0.8 mm or more |
| **7217 10 31 00** | 0.0% |  | - - - - Containing indentations, ribs, grooves or other deformations produced during the rolling process |
| **7217 10 39 00** |  |  | - - - - Other |
| **7217 10 50 00** |  |  | - - Containing by weight 0,25% or more but less than 0,6% of carbon |
| **7217 10 90** |  |  | - - Containing by weight 0,6% or more of carbon |
| **7217 10 90 10** |  |  | - - - Of non-alloy steel, with a maximum cross-sectional dimension exceeding 3 mm |
| **7217 10 90 90** |  |  | - - - Other |
| **7217 20** |  |  | **- Plated or coated with zinc** |
|  |  |  | - - Containing by weight less than 0,25% of carbon |
| **7217 20 10 00** |  |  | - - - With a maximum cross-sectional dimension of less than 0.8 mm |
| **7217 20 30 00** |  |  | - - - With a maximum cross-sectional dimension of 0.8 mm or more |
| **7217 20 50 00** |  |  | - - Containing by weight 0,25% or more but less than 0,6% of carbon |
| **7217 20 90** |  |  | - - Containing by weight 0,6% or more of carbon |
| **7217 20 90 10** |  |  | - - - Of non-alloy steel, with a maximum cross-sectional dimension exceeding 3 mm |
| **7217 20 90 90** |  |  | - - - Other |
| **7217 30** |  |  | **- Plated or coated with other base metals** |
|  |  |  | - - Containing by weight less than 0,25% of carbon |
| **7217 30 41 00** |  |  | - - - Copper-coated |
| **7217 30 49 00** |  |  | - - - Other |
| **7217 30 50 00** |  |  | - - Containing by weight 0,25% or more but less than 0,6% of carbon |
| **7217 30 90 00** |  |  | - - Containing by weight 0,6% or more of carbon |
| **7217 90** |  |  | **- Other** |
| **7217 90 20 00** |  |  | - - Containing by weight less than 0,25% of carbon |
| **7217 90 50 00** |  |  | - - Containing by weight 0,25% or more but less than 0,6% of carbon |
| **7217 90 90 00** |  |  | - - Containing by weight 0,6% or more of carbon |
|  |  |  | **III. STAINLESS STEEL** |
| **7218** |  |  | **Stainless steel in ingots or other primary forms; semi-finished products of stainless steel** |
| **7218 10 00 00** | 0.0% |  | **- Ingots and other primary forms** |
|  |  |  | **- Other** |
| **7218 91** |  |  | - - Of rectangular (other than square) cross-section |
| **7218 91 10 00** | 0.0% |  | - - - Containing by weight 2,5% or more of nickel |
| **7218 91 80 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7218 99** |  |  | - - Other |
|  |  |  | - - - Of square cross-section |
| **7218 99 11 00** | 0.0% |  | - - - - Rolled or obtained by continous casting |
| **7218 99 19 00** |  |  | - - - - Forged |
|  |  |  | - - - Other |
| **7218 99 20 00** |  |  | - - - - Rolled or obtained by continuous casting |
| **7218 99 80 00** |  |  | - - - - Forged |
| **7219** |  |  | **Flat-rolled products of stainless steel, of a width of 600 mm or more** |
|  |  |  | **- Not further worked than hot-rolled, in coils** |
| **7219 11 00 00** | 0.0% |  | - - Of a thickness exceeding 10 mm |
| **7219 12** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7219 12 10 00** | 0.0% |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 12 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 13** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7219 13 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 13 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 14** |  |  | - - Of a thickness of less than 3 mm |
| **7219 14 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 14 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
|  |  |  | **- Not further worked than hot-rolled, not in coils** |
| **7219 21** |  |  | - - Of a thickness exceeding 10 mm |
| **7219 21 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 21 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 22** |  |  | - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7219 22 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 22 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 23 00 00** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7219 24 00 00** |  |  | - - Of a thickness of less than 3 mm |
|  |  |  | **- Not further worked than cold-rolled (cold-reduced)** |
| **7219 31 00 00** |  |  | - - Of a thickness of 4.75 mm or more |
| **7219 32** |  |  | - - Of a thickness of 3 mm or more but less than 4.75 mm |
| **7219 32 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 32 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 33** |  |  | - - Of a thickness exceeding 1 mm but less than 3 mm |
| **7219 33 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 33 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 34** |  |  | - - Of a thickness of 0.5 mm or more but not exceeding 1 mm |
| **7219 34 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 34 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 35** |  |  | - - Of a thickness of less than 0.5 mm |
| **7219 35 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7219 35 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7219 90** |  |  | **- Other** |
| **7219 90 20 00** |  |  | - - Perforated |
| **7219 90 80 00** |  |  | - - Other |
| **7220** |  |  | **Flat-rolled products of stainless steel, of a width of less than 600 mm** |
|  |  |  | **- Not further worked than hot-rolled** |
| **7220 11 00 00** | 0.0% |  | - - Of a thickness of 4.75 mm or more |
| **7220 12 00 00** |  |  | - - Of a thickness of less than 4.75 mm |
| **7220 20** |  |  | **- Not further worked than cold-rolled (cold-reduced)** |
|  |  |  | - - Of a thickness of 3 mm or more, containing by weight |
| **7220 20 21 00** | 0.0% |  | - - - 2,5% or more of nickel |
| **7220 20 29 00** |  |  | - - - Less than 2,5% of nickel |
|  |  |  | - - Of a thickness exceeding 0.35 mm but of less than 3 mm, containing by weight |
| **7220 20 41 00** |  |  | - - - 2,5% or more of nickel |
| **7220 20 49 00** |  |  | - - - Less than 2,5% of nickel |
|  |  |  | - - Of a thickness not exceeding 0.35 mm, containing by weight |
| **7220 20 81 00** |  |  | - - - 2,5% or more of nickel |
| **7220 20 89 00** |  |  | - - - Less than 2,5% of nickel |
| **7220 90** |  |  | **- Other** |
| **7220 90 20 00** |  |  | - - Perforated |
| **7220 90 80 00** |  |  | - - Other |
| **7221** |  |  | **Bars and rods, hot-rolled, in irregularly wound coils, of stainless steel** |
| **7221 00 10 00** | 0.0% |  | **- Containing by weight 2,5% or more of nickel** |
| **7221 00 90 00** |  |  | **- Containing by weight less than 2,5% of nickel** |
| **7222** |  |  | **Other bars and rods of stainless steel; angles, shapes and sections of stainless steel** |
|  |  |  | **- Bars and rods, not further worked than hot-rolled, hot-drawn or extruded** |
| **7222 11** |  |  | - - Of circular cross-section |
|  |  |  | - - - Of a diameter of 80 mm or more, containing by weight |
| **7222 11 11 00** | 0.0% |  | - - - - 2,5% or more of nickel |
| **7222 11 19 00** |  |  | - - - - Less than 2,5% of nickel |
|  |  |  | - - - Of a diameter of less than 80 mm, containing by weight |
| **7222 11 81 00** |  |  | - - - - 2,5% or more of nickel |
| **7222 11 89 00** |  |  | - - - - Less than 2,5% of nickel |
| **7222 19** |  |  | - - Other |
| **7222 19 10 00** |  |  | - - - Containing by weight 2,5% or more of nickel |
| **7222 19 90 00** |  |  | - - - Containing by weight less than 2,5% of nickel |
| **7222 20** |  |  | **- Bars and rods, not further worked than cold-formed or cold-finished** |
|  |  |  | - - Of circular cross-section |
|  |  |  | - - - Of a diameter of 80 mm or more, containing by weight |
| **7222 20 11 00** |  |  | - - - - 2,5% or more of nickel |
| **7222 20 19 00** |  |  | - - - - Less than 2,5% of nickel |
|  |  |  | - - - Of a diameter of 25 mm or more, but less than 80 mm, containing by weight |
| **7222 20 21 00** |  |  | - - - - 2,5% or more of nickel |
| **7222 20 29 00** |  |  | - - - - Less than 2,5% of nickel |
|  |  |  | - - - Of a diameter of less than 25 mm, containing by weight |
| **7222 20 31 00** |  |  | - - - - 2,5% or more of nickel |
| **7222 20 39 00** |  |  | - - - - Less than 2,5% of nickel |
|  |  |  | - - Other, containing by weight |
| **7222 20 81 00** |  |  | - - - 2,5% or more of nickel |
| **7222 20 89 00** |  |  | - - - Less than 2,5% of nickel |
| **7222 30** |  |  | **- Other bars and rods** |
|  |  |  | - - Forged, containing by weight |
| **7222 30 51 00** |  |  | - - - 2,5% or more of nickel |
| **7222 30 91 00** |  |  | - - - Less than 2,5% of nickel |
| **7222 30 97** |  |  | - - Other |
| **7222 30 97 10** |  |  | - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7222 30 97 90** |  |  | - - - Other |
| **7222 40** |  |  | **- Angles, shapes and sections** |
| **7222 40 10 00** |  |  | - - Not further worked than hot-rolled, hot-drawn or extruded |
| **7222 40 50 00** |  |  | - - Not further worked than cold-formed or cold-finished |
| **7222 40 90** |  |  | - - Other |
| **7222 40 90 10** |  |  | - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7222 40 90 90** |  |  | - - - Other |
| **7223** |  |  | **Wire of stainless steel** |
|  |  |  | **- Containing by weight 2,5% or more of nickel** |
| **7223 00 11 00** | 0.0% |  | - - Containing by weight 28% or more but not more than 31% of nickel and 20% or more but not more than 22% of chromium |
| **7223 00 19 00** |  |  | - - Other |
|  |  |  | **- Containing by weight less than 2,5% of nickel** |
| **7223 00 91 00** |  |  | - - Containing by weight 13% or more but not more than 25% of chromium and 3,5% or more but not more than 6% of aluminium |
| **7223 00 99 00** |  |  | - - Other |
|  |  |  | **IV. OTHER ALLOY STEEL; HOLLOW DRILL BARS AND RODS, OF ALLOY OR NON-ALLOY STEEL** |
| **7224** |  |  | **Other alloy steel in ingots or other primary forms; semi-finished products of other alloy steel** |
| **7224 10** |  |  | **- Ingots and other primary forms** |
| **7224 10 10 00** | 0.0% |  | - - Of tool steel |
| **7224 10 90 00** |  |  | - - Other |
| **7224 90** |  |  | **- Other** |
| **7224 90 02** |  |  | - - Of tool steel |
| **7224 90 02 29** | 0.0% |  | - - - Of rectangular (including square) cross-section |
|  |  |  | - - - Other |
| **7224 90 02 89** | 0.0% |  | - - - - Hot-rolled or obtained by continuous casting |
| **7224 90 02 99** |  |  | - - - - Other |
|  |  |  | - - Other |
|  |  |  | - - - Of rectangular (including square) cross-section |
|  |  |  | - - - - Hot-rolled or obtained by continuous casting |
|  |  |  | - - - - - The width measuring less than twice the thickness |
| **7224 90 03 00** | 0.0% |  | - - - - - - Of high-speed steel |
| **7224 90 05 00** |  |  | - - - - - - Containing by weight not more than 0,7% of carbon, 0,5% or more but not more than 1,2% of manganese and 0,6% or more but not more than 2,3% of silicon; containing by weight 0,0008% or more of boron with any other element less than the minimum content referred to in note 1(f) to this chapter |
| **7224 90 07 00** |  |  | - - - - - - Other |
| **7224 90 14 00** |  |  | - - - - - Other |
| **7224 90 18 00** |  |  | - - - - Forged |
|  |  |  | - - - Other |
|  |  |  | - - - - Hot-rolled or obtained by continuous casting |
| **7224 90 31 00** |  |  | - - - - - Containing by weight not less than 0,9% but not more than 1,15% of carbon, not less than 0,5% but not more than 2% of chromium and, if present, not more than 0,5% of molybdenum |
| **7224 90 38 00** |  |  | - - - - - Other |
| **7224 90 90 00** |  |  | - - - - Forged |
| **7225** |  |  | **Flat-rolled products of other alloy steel, of a width of 600 mm or more** |
|  |  |  | **- Of silicon-electrical steel** |
| **7225 11** |  |  | - - Grain-oriented |
|  |  |  | - - - Of a thickness exceeding 0.16 mm |
| **7225 11 00 11** | 0.0% |  | - - - - With a maximum core loss not higher than 0.9 W/kg |
| **7225 11 00 15** |  |  | - - - - With a maximum core loss higher than 0.9 W/kg but not higher than 1.05 W/kg |
| **7225 11 00 19** |  |  | - - - - With a maximum core loss higher than 1.05 W/kg |
| **7225 11 00 90** |  |  | - - - Other |
| **7225 19** |  |  | - - Other |
| **7225 19 10** |  |  | - - - Hot-rolled |
| **7225 19 10 10** |  |  | - - - - Products clad, plated or coated, not in coils, without patterns in relief, of a thickness exceeding 10 mm and products clad, plated or coated, not in coils, without patterns in relief, of a thickness of 4.75 mm or more but not exceeding 10 mm and of a width of 2 050 mm or more |
| **7225 19 10 90** |  |  | - - - - Other |
| **7225 19 90 00** |  |  | - - - Cold-rolled |
| **7225 30** |  |  | **- Other, not further worked than hot-rolled, in coils** |
| **7225 30 10 00** |  |  | - - Of tool steel |
| **7225 30 30** |  |  | - - Of high-speed steel |
| **7225 30 30 10** |  |  | - - - Not further worked than rolled; not further worked than surface-treated, including cladding or simply cut into shapes other than rectangular (including square) |
| **7225 30 30 90** |  |  | - - - Other |
| **7225 30 90 00** |  |  | - - Other |
| **7225 40** |  |  | **- Other, not further worked than hot-rolled, not in coils** |
| **7225 40 12 00** |  |  | - - Of tool steel |
| **7225 40 15 00** |  |  | - - Of high-speed steel |
|  |  |  | - - Other |
| **7225 40 40 00** |  |  | - - - Of a thickness exceeding 10 mm |
| **7225 40 60** |  |  | - - - Of a thickness of 4.75 mm or more but not exceeding 10 mm |
| **7225 40 60 10** |  |  | - - - - Of a width of 2 050 mm or more |
| **7225 40 60 90** |  |  | - - - - Other |
| **7225 40 90 00** |  |  | - - - Of a thickness of less than 4.75 mm |
| **7225 50** |  |  | **- Other, not further worked than cold-rolled (cold-reduced)** |
| **7225 50 20** |  |  | - - Of high-speed steel |
| **7225 50 20 10** |  |  | - - - Not further worked than rolled; not further worked than surface-treated, including cladding or simply cut into shapes other than rectangular (including square) |
| **7225 50 20 90** |  |  | - - - Other |
| **7225 50 80 00** |  |  | - - Other |
|  |  |  | **- Other** |
| **7225 91** |  |  | - - Electrolytically plated or coated with zinc |
| **7225 91 00 10** |  |  | - - - Not further worked than surface-treated, including cladding or simply cut into shapes other than rectangular (including square) |
| **7225 91 00 90** |  |  | - - - Other |
| **7225 92** |  |  | - - Otherwise plated or coated with zinc |
| **7225 92 00 20** |  |  | - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7225 92 00 80** |  |  | - - - Other |
| **7225 99** |  |  | - - Other |
|  |  |  | - - - Not further worked than surface-treated, including cladding or simply cut into shapes other than rectangular (including square) |
| **7225 99 00 11** |  |  | - - - - Painted, varnished or coated with plastics on at least one side, excluding products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70% or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7225 99 00 22** |  |  | - - - - Other, aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7225 99 00 25** |  |  | - - - - Other |
| **7225 99 00 40** |  |  | - - - Other, of a thickness exceeding 10 mm or of a thickness of 4.75 mm or more but not exceeding 10 mm and of a width of 2 050 mm or more |
|  |  |  | - - - Other |
| **7225 99 00 91** |  |  | - - - - Painted, varnished or coated with plastics on at least one side, excluding so-called "sandwich panels" of a kind used for building applications and consisting of two outer metal sheets with a stabilising core of insulation material sandwiched between them, excluding those products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70% or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7225 99 00 92** |  |  | - - - - Other, aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7225 99 00 95** |  |  | - - - - Other |
| **7226** |  |  | **Flat-rolled products of other alloy steel, of a width of less than 600 mm** |
|  |  |  | **- Of silicon-electrical steel** |
| **7226 11** |  |  | - - Grain-oriented |
|  |  |  | - - - Of a width exceeding 500 mm |
|  |  |  | - - - - Of a thickness exceeding 0.16 mm |
| **7226 11 00 12** | 0.0% |  | - - - - - With a maximum core loss not higher than 0.9 W/kg |
| **7226 11 00 14** |  |  | - - - - - With a maximum core loss higher than 0.9 W/kg but not higher than 1.05 W/kg |
| **7226 11 00 16** |  |  | - - - - - With a maximum core loss higher than 1.05 W/kg |
| **7226 11 00 19** |  |  | - - - - Other |
|  |  |  | - - - Of a width not exceeding 500 mm |
|  |  |  | - - - - Of a thickness exceeding 0.16 mm |
| **7226 11 00 92** |  |  | - - - - - With a maximum core loss not higher than 0.9 W/kg |
| **7226 11 00 94** |  |  | - - - - - With a maximum core loss higher than 0.9 W/kg but not higher than 1.05 W/kg |
| **7226 11 00 96** |  |  | - - - - - With a maximum core loss higher than 1.05 W/kg |
| **7226 11 00 99** |  |  | - - - - Other |
| **7226 19** |  |  | - - Other |
| **7226 19 10** |  |  | - - - Not further worked than hot-rolled |
| **7226 19 10 10** |  |  | - - - - Products clad, plated or coated |
| **7226 19 10 90** |  |  | - - - - Other |
| **7226 19 80** |  |  | - - - Other |
| **7226 19 80 10** |  |  | - - - - Of a width exceeding 500 mm |
| **7226 19 80 90** |  |  | - - - - Of a width not exceeding 500 mm |
| **7226 20** |  |  | **- Of high-speed steel** |
| **7226 20 00 20** |  |  | - - Products further worked than hot rolled, or clad, plated or coated |
| **7226 20 00 95** |  |  | - - Other |
|  |  |  | **- Other** |
| **7226 91** |  |  | - - Not further worked than hot-rolled |
| **7226 91 20 00** |  |  | - - - Of tool steel |
|  |  |  | - - - Other |
| **7226 91 91 00** |  |  | - - - - Of a thickness of 4.75 mm or more |
| **7226 91 99 00** |  |  | - - - - Of a thickness of less than 4.75 mm |
| **7226 92** |  |  | - - Not further worked than cold-rolled (cold-reduced) |
| **7226 92 00 10** |  |  | - - - Of a width exceeding 500 mm |
| **7226 92 00 90** |  |  | - - - Of a width not exceeding 500 mm |
| **7226 99** |  |  | - - Other |
| **7226 99 10 00** |  |  | - - - Electrolytically plated or coated with zinc |
| **7226 99 30** |  |  | - - - Otherwise plated or coated with zinc |
| **7226 99 30 10** |  |  | - - - - Aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7226 99 30 90** |  |  | - - - - Other |
| **7226 99 70** |  |  | - - - Other |
|  |  |  | - - - - Of a width not exceeding 500 mm, hot-rolled, not further worked than clad; of a width exceeding 500 mm, not further worked than surface-treated, including cladding |
| **7226 99 70 11** |  |  | - - - - - Painted, varnished or coated with plastics on at least one side, excluding products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70% or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7226 99 70 19** |  |  | - - - - - Other |
|  |  |  | - - - - Other |
| **7226 99 70 91** |  |  | - - - - - Painted, varnished or coated with plastics on at least one side, excluding so-called "sandwich panels" of a kind used for building applications and consisting of two outer metal sheets with a stabilising core of insulation material sandwiched between them, excluding those products with a final coating of zinc-dust (a zinc-rich paint, containing by weight 70% or more of zinc) and excluding products with a substrate with a metallic coating of chromium or tin |
| **7226 99 70 94** |  |  | - - - - - Other, aluminium killed; plated or coated by hot dip galvanisation with zinc and/or with aluminium, and no other metal; chemically passivated; containing by weight: 0.015% or more but not more than 0.170% of carbon, 0.015% or more but not more than 0.100% of aluminium, not more than 0.045% of niobium, not more than 0.010% of titanium and not more than 0.010% of vanadium; presented in coils, cut-to-length sheets and narrow strips |
| **7226 99 70 96** |  |  | - - - - - Other |
| **7227** |  |  | **Bars and rods, hot-rolled, in irregularly wound coils, of other alloy steel** |
| **7227 10 00 00** | 0.0% |  | **- Of high-speed steel** |
| **7227 20 00 00** |  |  | **- Of silico-manganese steel** |
| **7227 90** |  |  | **- Other** |
| **7227 90 10 00** | 0.0% |  | - - Containing by weight 0,0008% or more of boron with any other element less than the minimum content referred to in note 1(f) to this chapter |
| **7227 90 50 00** |  |  | - - Containing by weight 0,9% or more but not more than 1,15% of carbon, 0,5% or more but not more than 2% of chromium and, if present, not more than 0,5% of molybdenum |
| **7227 90 95 00** |  |  | - - Other |
| **7228** |  |  | **Other bars and rods of other alloy steel; angles, shapes and sections, of other alloy steel; hollow drill bars and rods, of alloy or non-alloy steel** |
| **7228 10** |  |  | **- Bars and rods, of high-speed steel** |
| **7228 10 20 00** | 0.0% |  | - - Not further worked than hot-rolled, hot-drawn or extruded; hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 10 50 00** |  |  | - - Forged |
| **7228 10 90 00** |  |  | - - Other |
| **7228 20** |  |  | **- Bars and rods, of silico-manganese steel** |
| **7228 20 10** |  |  | - - Of rectangular (other than square) cross-section, hot-rolled on four faces |
| **7228 20 10 10** | 0.0% |  | - - - Not further worked than hot-rolled, hot-drawn or extruded |
|  |  |  | - - - Other |
| **7228 20 10 91** | 0.0% |  | - - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 20 10 99** |  |  | - - - - Other |
|  |  |  | - - Other |
| **7228 20 91 00** |  |  | - - - Not further worked than hot-rolled, hot-drawn or extruded; hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 20 99 00** |  |  | - - - Other |
| **7228 30** |  |  | **- Other bars and rods, not further worked than hot-rolled, hot-drawn or extruded** |
| **7228 30 20** |  |  | - - Of tool steel |
| **7228 30 20 10** |  |  | - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 20 90** |  |  | - - - Other |
|  |  |  | - - Containing by weight 0,9% or more but not more than 1,15% of carbon, 0,5% or more but not more than 2% of chromium and, if present, not more than 0,5% of molybdenum |
| **7228 30 41** |  |  | - - - Of circular cross-section of a diameter of 80 mm or more |
| **7228 30 41 10** |  |  | - - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 41 90** |  |  | - - - - Other |
| **7228 30 49** |  |  | - - - Other |
| **7228 30 49 10** |  |  | - - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 49 90** |  |  | - - - - Other |
|  |  |  | - - Other |
|  |  |  | - - - Of circular cross-section, of a diameter of |
| **7228 30 61** |  |  | - - - - 80 mm or more |
| **7228 30 61 10** | 0.0% |  | - - - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 61 90** |  |  | - - - - - Other |
| **7228 30 69** |  |  | - - - - Less than 80 mm |
| **7228 30 69 10** |  |  | - - - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 69 90** |  |  | - - - - - Other |
| **7228 30 70** |  |  | - - - Of rectangular (other than square) cross-section, hot-rolled on four faces |
| **7228 30 70 10** |  |  | - - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 70 90** |  |  | - - - - Other |
| **7228 30 89** |  |  | - - - Other |
| **7228 30 89 10** |  |  | - - - - High fatigue performance concrete reinforcing bars and rods, containing indentations, ribs, grooves or other deformations produced during the rolling process or twisted after rolling |
| **7228 30 89 90** |  |  | - - - - Other |
| **7228 40** |  |  | **- Other bars and rods, not further worked than forged** |
| **7228 40 10 00** |  |  | - - Of tool steel |
| **7228 40 90 00** |  |  | - - Other |
| **7228 50** |  |  | **- Other bars and rods, not further worked than cold-formed or cold-finished** |
| **7228 50 20 00** |  |  | - - Of tool steel |
| **7228 50 40 00** |  |  | - - Containing by weight 0,9% or more but not more than 1,15% of carbon, 0,5% or more but not more than 2% of chromium and, if present, not more than 0,5% of molybdenum |
|  |  |  | - - Other |
|  |  |  | - - - Of circular cross-section, of a diameter of |
| **7228 50 61 00** |  |  | - - - - 80 mm or more |
| **7228 50 69 00** |  |  | - - - - Less than 80 mm |
| **7228 50 80 00** |  |  | - - - Other |
| **7228 60** |  |  | **- Other bars and rods** |
| **7228 60 20** |  |  | - - Of tool steel |
| **7228 60 20 10** |  |  | - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 60 20 90** |  |  | - - - Other |
| **7228 60 80** |  |  | - - Other |
| **7228 60 80 10** |  |  | - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 60 80 90** |  |  | - - - Other |
| **7228 70** |  |  | **- Angles, shapes and sections** |
| **7228 70 10 00** |  |  | - - Not further worked than hot-rolled, hot-drawn or extruded |
| **7228 70 90** |  |  | - - Other |
| **7228 70 90 10** |  |  | - - - Hot-rolled, hot-drawn or extruded, not further worked than clad |
| **7228 70 90 90** |  |  | - - - Other |
| **7228 80 00 00** |  |  | **- Hollow drill bars and rods** |
| **7229** |  |  | **Wire of other alloy steel** |
| **7229 20 00 00** | 0.0% |  | **- Of silico-manganese steel** |
| **7229 90** |  |  | **- Other** |
| **7229 90 20 00** | 0.0% |  | - - Of high-speed steel |
| **7229 90 50 00** |  |  | - - Containing by weight 0,9% or more but not more than 1,15% of carbon, 0,5% or more but not more than 2% of chromium and, if present, not more than 0,5% of molybdenum |
| **7229 90 90 00** |  |  | - - Other |