### Chapter Notes

For the purposes of heading 4702, the expression 'chemical wood pulp, dissolving grades' means chemical wood pulp having by weight an insoluble fraction of 92% or more for soda or sulphate wood pulp or of 88% or more for sulphite wood pulp after one hour in a caustic soda solution containing 18% sodium hydroxide (NaOH) at 20 °C, and for sulphite wood pulp an ash content that does not exceed 0.15% by weight.